Demo requires two Raspberries Pi Pico 2. One to render and display graphics and the other one to stream music from sd card. 
Copy both wav files to sd card and place it in Raspberry with audio_corpsetravel.uf2
File video_corpsetravel.uf2 must be in RPI with display based on ST7789VW.